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Specification


Part 1 – General

1.01 Work Included

A. Supply of material, tools, and other equipment necessary to carry out the installation of the floating floor as shown on drawings.

1.02 System Description

A. The floating floors shall be elastically suspended from the structural floor, using flexible floor mounts. The floor mounts shall be embedded in the concrete when the concrete is poured and once the concrete is cured the slab shall be lifted using the jack-up system of the floor mounts.

1.03 Quality

A. The manufacturing of the floor mounts shall be performed in a way that it fulfills its function as well as to comply with all applicable regulations.

1.04 Submittals

A. Product CAD drawings shall be provided to the designer for approval.

B. Product performance data shall be submitted to the designer for review and shall include an Airborne Sound Insulation Report according to ISO 10140-2 and an Impact Sound Level Report according to ISO 10140-3. The tests shall be performed in an independent laboratory. Test reports shall document a minimum Sound Transmission Class (STC) 72 and a minimum Impact Isolation Class (IIC) 69 for a resiliently suspended 4” thick floating slab, 1” air gap and a normalized 6” reinforced concrete structure. 
Part 2 – Products

2.01 Materials

A. The floating floor mounts shall be designed and manufactured by AMC MECANOCAUCHO®.

B. The floating floor mounts shall be able to continuously withstand the weight of the floating floor without suffering any significant settling after initial deflection.

C. The floating floor mount model shall be chosen to provide a natural frequency less than 15Hz.




Part 3 – Execution

3.01 Installation

A. The surface of the structural floor shall be flat, smooth and cleared of debris.

B. The floating slab shall have reinforcing bars inside it.

C. In places where rigid contact between the floating floor and other non-elastically 
suspended elements is present, elastic materials shall be used to avoid/eliminate the rigid connection that act as acoustic bridges.

D. Once the concrete slab is cured, it shall be raised turning the leveling stud bolts up to the design height. Incorrect raising procedures might cause cracks in the slab.

E. The installation of all sound isolation materials specified herein, shall be in accordance with procedures submitted by the isolation material manufacturer and approved by the architect.
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